Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**1)** PPE is the first line of defense against eye and face hazards.

A. True

B. False

**2)** Assure that eye protection is \_\_\_\_\_\_ approved.

A. ANSI A14

B. ANSI Z87

C. ASTM F17

D. ASTM A391

**3)** Choose all that apply. Recurring training is required for the following situations?

A. Monthly, as a refresher

B. If a new hazard is introduced

C. If the job changes in some way

D. If the employee is seen to be wearing PPE incorrectly

**4)** Choose all that apply. Employees must be trained in which of the following areas?

A. When to use PPE

B. What PPE is necessary

C. Proper care and maintenance of PPE

D. The useful life of PPE

E. Use of PPE

F. Limitations of PPE

G. None of the above

**5)** Which of the following requires ventilation?

A. A face shield

B. Safety glasses

C. Safety goggles

D. None of the above

**6)** Ordinary corrective eyewear can be worn to protect against hazards to the eyes.

A. True

B. False

**7)** Choose all that apply. Which hazards do safety glasses shield the wearer’s eyes from?

A. Dust

B. Objects

C. Chemicals

D. Flying fragments

**8)** Choose all that apply. Workers handling corrosive chemicals such as acids should be wearing the following PPE for eye and face protection.

1. Face shield
2. Specialized chemical goggles
3. Specialized chemical safety glasses

**9)** In order to select the proper shading of lens you must know the type and degree of radiant energy in the workplace.

A. True

B. False

**10)** Welding helmets must be worn by welding observers.

A. True

B. False

**11)** The higher the shade number, the more light radiation can pass through the lens.

A. True

B. False

**Answer Key**

1. B

2. B

3. B, C & D

4. A, B, C, D, E & F

5. C

6. B

7. B & D

8. A & B

9. A

10. A

11. B